### SININTOUT

sets the interpolation factor of the encoder equivalent output in case of sine encoder option board, software sine encoder interface, or software resolver interface.

For sine encoder systems, the encoder output value (ENCOUT) = MENCRES * SININTOUT / ENCOUTO.

Firmware Versions: 3.3.0 and later
Type: switch mode (R/W) Range: 1, 2, 4, 8, 16, 32, 64, 128
Units: n/a Default: 1
Opmodes: all Drive Status: dis EEPROM: yes