### ABSPOSMOD

used to set the way to handle absolute position from ENDAT encoder. Possible values:
0 - Handle absolute position as unsigned value
1 - Handle absolute position as signed value
2 - Handle absolute position as unsigned value, reversed direction.
3 - Handle absolute position as signed value, reversed direction.

Firmware Versions: 6.5.3
Type: (R/W) Range: 0 , 1
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: yes