### ICOFF

sets the user value of the current offset of phase C.
When queried, returns the actual (presently used) current phase C offset.
AUTONULL command was expanded to accept the value 2. When AUTONULL=2 the current phase offset is taken from user variables IAOFF and ICOFF. In AUTONULL=0,1 , IAOFF and ICOFF display the offset values set by the automatic current nulling.

Firmware Versions: 4.1.0
Type: variable (R/W) Range: -1000 to 1000
Units: % of DIPEAK * 0.1 Default: 0
Opmodes: all Drive Status: en/dis EEPROM: yes