### ENCOUT

sets the resolution (number of lines) of the encoder equivalent output channel for resolver based systems only. For
encoder-based systems, this variable is read-only and is set equal to MENCRES (for firmware versions prior to
3.3.0) or MENCRES / ENCOUTO (for firmware versions 3.3.0 and later). For sine encoder-based systems, this
variable is read-only and is set equal to MENCRES * SININTOUT / ENCOUTO.
Note that ENCOUT values of 2048 and 4096 are available only when VLIM < 6100 RPM (RDRES = 14 or 16).
ENCOUT values of 8192 and 16384 are available only when VLIM <=1500 RPM (RDRES = 16). In the majority
of resolvers, one electrical revolution = one mechanical revolution.

Firmware Versions: all
Type: switch mode (R/W) Range: 512, 1024, 2048, 4096, 8192, or 16384
Units: lines per electrical Default: 1024
rev. of the resolver
Opmodes: all Drive Status: dis EEPROM: yes