### MLMAX

Appears in the command list, but has no function in the drive. Used to be motor line to line maximum induction.
Sets the motor’s maximum line-to-line inductance. This variable is used for current loop controller design and as an input to the Torque Angle Control algorithms. When this variable is changed, the drive will enter a no-comp state, requiring a CONFIG command.
See CONFIG and MLMIN commands.

Firmware Versions: all
Type: variable (R/W) Range: 0 to 32767
Units: millihenries *10^-2 Default: motor data
Opmodes: all Drive Status: dis EEPROM: yes