### RSTVAR

sets the all operational variables, switch variables, and switch mode variables to their factory default settings. These settings are stated within this document under the variable DEFAULT category. The default values of variables loaded from a motor data file cannot be predicted and are denoted "motor data" in the DEFAULT category.

Firmware Versions: all
Command Syntax: RSTVAR
Opmodes: all Drive Status: dis