### FOLDD

sets the delay time for drive foldback. This is the amount of time that the system current can exceed ICONT before the drive will enter the foldback state (FOLD=1). The time units assume a worst-case scenario where the drive is applying DIPEAK current. A current level of less than DIPEAK can be allowed for longer time. See also FOLD, FOLDT, FOLDR, FOLDMODE, FOLDTIME, MFOLD, MFOLDDIS, MFOLDR, and MFOLDT.

Firmware Versions: all
Type: variable (R/W) Range: 1 to 32767
Units: milli-seconds at DIPEAK Default: drive data
Opmodes: all Drive Status: en/dis EEPROM: yes