### ANOUTVAL

Write user value to DAC1 (analog output at user I/O connector) for ANOUT=6, or DAC2 (internal analog output). Serial interface writes and reads the user value for DAC1 only. SERCOS interface writes and reads the user value for DAC1 and DAC2.

Firmware Versions: 6.5.9
Type: (R/W) Range: DAC: 1, 2. Value: -32768 to 32767
Units: n/a Default: n/a
Opmodes: all Drive Status: en/dis EEPROM: no