### VLIM2

sets the application velocity limit, allowing the user to limit the motor’s peak velocity in addtion to limiting current command and VLIM. When VFI input is inactive , saturation is VLIM. When the input is active the value decreases according to VLIM2.

See VLIM command.

Firmware Versions: 7.4.6
Type: variable (R/W) Range: 10 to VMAX
Units: rotary: RPM Default: VMAX
linear: mm/sec
Opmodes: all Drive Status: dis EEPROM: yes