### FOLDR

sets the recovery time for drive foldback. After the drive enters the foldback state (FOLD=1), and the current folds back to ICONT, this is the minimum amount of time that the current should be held at 0 before it is allowed to be DIPEAK for full FOLDD time again. See also FOLD, FOLDD, FOLDT, FOLDMODE, FOLDTIME, MFOLD, MFOLDD, MFOLDDIS, and MFOLDT.

Firmware Versions: all
Type: variable (R/W) Range: 1 to 32767
Units: milli-seconds Default: drive data
Opmodes: all Drive Status: en/dis EEPROM: yes