### FLTHIST

will cause the drive to transmit the fault history buffer to the serial port. The most recent fault is sent first. Up to 10 fault messages will be output by the drive, with each fault message followed by a CR-LF. A time stamp in the format of hours:minutes is displayed along with each fault, indicating the time at which the fault occurred (refer to TRUN for more time stamp info).

Firmware Versions: all
Command Syntax: FLTHIST
Opmodes: all Drive Status: en/dis