### C6 - Internal Flex Cable (Flat cable connecting power stage to digital board)

Pin No. | Function
1 | Q1+
2 | Q2+
3 | DGND
4 | DGND
5 | Q3+
6 | Q4+
7 | DGND
8 | DGND
9 | Q5+
10 | Q6+
11 | +5VDC
12 | +5VDC
13 | DRVTMP
14 | /OC
15 | /OV
16 | /UV
17 | PWRID0
18 | PWRID1
19 | PWRID2
20 | PWRID3
21 | Enc5V
22 | Enc5V
23 | V BUS
24 |
25 | -12V
26 | +12V
27 | IA RET
28 | IACTA
29 | IC RET
30 | IACTC

App Note:

White Papers:

> CD Series 5 Power stage