### RECRDY

indicates the ready status of the RECORD function. This variable can be polled after a RECORD command is issued to determine if the system is waiting for RECTRIG.
0 = RECTRIG has been received and record function is armed
1 = record function is waiting to be armed by RECTRIG command

Firmware Versions: all
Type: switch (R) Range: 0, 1
Units: n/a Default: 1
Opmodes: all Drive Status: en/dis EEPROM: no