### RECUI

Special recording from DSP memory locations. Factory record feature.

Syntax: RECUI <gap> <points> [<num>]
<gap> - record gap, like in regular RECORD. Range: 1 to 10000. (* 0.5 milliseconds).
<points> - number of recording points, like in regular record. Range: 1 to 340.
<num> - optional. Number of ui parameters to record. Range: 1 to 4. If not specified, the number of ui parameters to record is 4.

For internal use (debug).
Firmware Versions: all