### TEMPM

reads indirectly the motor temperature. Actually, it reads the voltage level of the circuit that converts the motor thermostat resistance into voltage.

Knowing the converting circuit (details upon request) and the voltage level yields the thermostat resistance.

Knowing the thermostat characteristics and the thermostat resistance yields the motor temperature.

Firmware Versions: 4.1.9 and later
Type: variable (R) Range: 0 to 5000
Units: millivolts Default: n/a
Opmodes: all Drive Status: en/dis EEPROM: no