### ENCOUTMOD

pulse up/pulse down mode added with ENCOUTMOD command.
0 - encoder simulation A/B (default).
1 - encoder simulation pulse up pulse down.
2 - added due to ucb1 - ucb2 compatibility issues
encoutmod 2
which inverts AqB<-->BqA was added. in sw sine encoutmod
default is 2
and in sw resolver encoutmod default is 0 (again to keep compatibility)

Firmware Versions: 6.1.0
Type: switch mode (R/W) Range: 0 to 2
Units: none Default: 0 - Resolver ; 2 - Encoder, Sine-Encoder
Opmodes: all Drive Status: dis EEPROM: yes