### RDRES

displays the resolver resolution on resolver-based systems. RDRES is a read-only variable which is automatically calculated in order to achieve maximum resolution. The setting is based on VLIM, which is the maximum application velocity. The relationship between VLIM and RDRES is given below:
if (VLIM ³ 6101) then RDRES = 12
if (1501 £ VLIM £ 6100) then RDRES = 14
if (VLIM £ 1500) then RDRES = 16

Firmware Versions: all
Type: switch mode (R) Range: 12, 14, or 16
Units: bits Default: n/a
Opmodes: all Drive Status: en/dis EEPROM: no