### THERMODE

determines the operation of the drive when the Motor Thermostat Input (THERM) opens.
0 = disable drive and open fault relay immediately
1 = disable drive after 2 minutes; open fault relay immediately
2 = do not disable drive; open fault relay immediately
3 = ignore thermostat input
4 = issue warning; no other action*
5 = issue warning, open fault relay after THERMTIME elapses*
Note: opening the fault relay sets RELAY=0.
* Firmware versions 3.1.0 and later

Firmware Versions: all
Type: switch mode (R/W) Range: 0 to 5
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: yes