### ICONT

sets the system continuous current. This variable is used in the foldback algorithm (see FOLD and FOLDMODE). The default value of this variable is the minimum of DICONT (Drive Continuous Current) and MICONT (Motor Continuous Current), unless that value exceeds IMAX, in which case ICONT will be set equal to IMAX. This variable will be reset to its default whenever DICONT or MICONT is changed. The user can override the default.

Firmware Versions: all
Type: variable (R/W) Range: 0 to IMAX
Units: % of DIPEAK *0.1 Default: min of DICONT and MICONT
Opmodes: all Drive Status: en/dis EEPROM: yes