### BIT

HPC peek and poke command for a specific bit.
Syntax:

bit haddr bit - querries the hexadecimal address "addr".
bit haddr
Use MEMB in order to verify the address.
bit value - Sets the "value" into "bit" of the "addr" address.

bit - ranges from 0 to 7
value - is 0 or 1

The file.xrr appearing in the UCB version directory is used for finding variables addresses.
See also: MEMB , DMEM , DMEMW, MEMW

Firmware Versions: all
Command Syntax: See above
Opmodes: all , Drive Status: en/dis