### DIVISIONS

Sets the number of divisions used for indexing (divides PROTARY). Allows the drive to operate as a division head. Activation is done by setting MODMODE=1 and configuring the INxMODE to 22 or 23. The velocity of the movement is determined by MISPEED0. Negative value of DIVISIONS indicate CCW direction.

Firmware Versions: From 3.7.0
Type: switch mode (R/W) Range: 2..32767 and -32767..-2
Units: n/a , Default: 4
Opmodes: all , Drive Status: en/dis , EEPROM: yes