### SININITST

queries the status of the sine calibration process. The possible values are:

0 = no request

1 = process running

2 = motor velocity too high The sine frequency cannot exceed 250Hz. When speed is reduced, the status returns to 1 (running).

3 = process complete

4 = defaults loaded Defaults are loaded when the calibration process has never been performed (in a new drive).

5 = internal failure

Firmware Versions: 6.2.0 and later
Type: variable (R)

Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: no