### ENCOUTO

sets the value of a scale-down factor for the encoder equivalent output channel (ENCOUT) for encoder- and sine
encoder-based systems only. For encoder-based systems with firmware versions 3.3.0 or later, ENCOUT =
MENCRES / ENCOUTO. For sine encoder-based systems, ENCOUT = MENCRES * SININTOUT / ENCOUTO.

Firmware Versions: all
Type: switch mode (R/W) Range: 1, 2, 4, 8, 16
Units: none Default: 1
Opmodes: all Drive Status: dis EEPROM: yes