### PRBMODE

is a switch mode variable that specifies the PRB excitation generator mode of operation.
0 - disabled (not activated).
1 - activated during recording (starting at RECORD trigger , see RECTRIG).
2 - activated immediately (free run).
Enable to disable transition resets PRBMODE to zero.

Type: Variable (R/W) Range: 0 to 2
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: no