### FOLD

displays the status of the drive foldback mechanism. When the system current level exceeds ICONT for too long, the drive enters foldback mode, FOLD changes from 0 to 1, and the drive current is limited gradually (in exponential fashion) to the value of ICONT. See also FOLDMODE, MFOLD, MFOLDD, MFOLDDIS, MFOLDR, and MFOLDT.
0 = motor foldback OFF
1 = motor foldback ON

Firmware Versions: all
Type: switch (R) Range: 0, 1
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: no