### SERIALNO

indicates the serial number of the drive in which the firmware is installed. This variable is included in the VER string. The serial number string variable MUST BE PRECEDED BY DOUBLE QUOTES (") when entered.

This variable is password protected.

Firmware Versions: all
Type: string variable (R/W) Range: 10 ASCII characters
Units: n/a Default: blanks
Opmodes: all Drive Status: en/dis EEPROM: yes