### DIPEAK

defines the peak rated current of the drive (sinusoidal RMS). This is a hardware-defined read-only variable. DIPEAK sets the 100% reference for several other current variables.

(*) Exception : in user defined HW configuration, DIPEAK can be set by the user.

Firmware Versions: all
Type: variable (R) Range: 20 to 2200
Units: amperes * 0.1 Default: hardware/user defined
Opmodes: all Drive Status: dis EEPROM: yes