### ENCINITST

displays the status of the encoder initialization function (see ENCINIT). This variable is reset to 0 when the user manually sets the index position (see MENCOFF).
0 = initialization process has not begun
1 = encoder initialization is in progress
2 = encoder initialization has been completed

Firmware Versions: all
Type: switch mode (R) Range: 0, 1, 2
Units: n/a Default: n/a
Opmodes: all Drive Status: en/dis EEPROM: no