### STOPPED

is a read-only switch that indicates the status of a move command (MA, MI, or MH) issued by the profile generator in Opmode 8. This bit will read 1 when a move is complete and the next move command can be issued. It will read 0 when a move is in progress.
0 = move in progress.
1 = move complete; next move command can be issued.

Firmware Versions: 3.1.0 and later
Type: switch (R) Range: 0, 1
Units: n/a Default: n/a
Opmodes: 8 Drive Status: en/dis EEPROM: n/a