### MFOLD

displays the status of the motor foldback circuit. When the system current level exceeds MICONT for too long, the drive enters motor foldback mode, MFOLD changes from 0 to 1, and the drive current is limited gradually (in exponential fashion) to the value of MICONT. See also FOLD, FOLDMODE, MFOLDD, MFOLDDIS, MFOLDR, and MFOLDT.
0 = motor foldback OFF (inactive)
1 = motor foldback ON (drive is limiting output current)

Firmware Versions: 3.2.0 and later
Type: switch (R) Range: 0, 1
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: no