### DECSTOP

is a deceleration that is used by drive commands that require a faster than usual stop. This DECSTOP value is used instead of DEC in the following instances: end-travel limits, HOLD, S, and a fault occurrence with ACTFAULT = 1. See also DISSPEED and DISTIME.

Firmware Versions: all
Type: variable (R/W) Range: 1 to 32767
Units: rotary: RPM * 1000/sec Default: 5000
linear: m/sec/sec
Opmodes: all Drive Status: en/dis EEPROM: yes