### DISTIME

sets the amount of time to wait after motor speed goes below DISSPEED before the drive is disabled in the Active Disable process. Once motor speed goes below DISSPEED, the drive will wait for the time period specified by DISTIME, and will then disable the drive. See also ACTFAULT, DECSTOP, DISTIME, and O1MODE=5.
Note that for using the Active Disable function effectively, a position controller has to configured.

Firmware Versions: 2.1.0 and later
Type: variable (R/W) Range: 0 to 65535
Units: millisecond * 0.1 Default: 100
Opmodes: all Drive Status: en/dis EEPROM: yes