### DICONT

defines the continuous rated current for the drive (sinusoidal RMS). This is a hardware-defined read-only variable that is detected automatically by the drive.

DICONT is usually 50% of DIPEAK, the peak current of the drive (this will not be true in many cases with the ServoStar CD). In a given application, the drive may be configured to a lower rating than DICONT by setting the value of ICONT to the desired rating.

(*) Exception : in user defined HW configuration, DICONT can be set by the user.

Firmware Versions: all
Type: variable (R) Range: 10 to 1100
Units: amperes * 0.1 Default: hardware/user defined
Opmodes: all Drive Status: dis EEPROM: yes