### DIPEN

displays the state of the Dip Switch Enable status (switch number 8 of the DIP switches on top of the drive). This variable has to be set=1 (switch set OFF) to allow the drive to be enabled.

0 = dip switch in disable state
1 = dip switch in enable state

Firmware Versions: all
Type: switch (R) Range: 0, 1
Units: n/a Default: hardware defined
Opmodes: all Drive Status: en/dis EEPROM: no