### MFOLDD

sets the delay time for motor foldback. This is the amount of time that the system current can exceed MICONT before the drive will enter the motor foldback state (MFOLD=1). The time units assume a worst-case scenario where the drive is applying MIPEAK current. A current level of less than MIPEAK can be allowed for longer time. See also FOLD, FOLDD, FOLDR, FOLDT, FOLDMODE, FOLDTIME, MFOLD, MFOLDDIS, MFOLDR, and MFOLDT.

Firmware Versions: 3.2.0 and later
Type: variable (R/W) Range: 1 to 2400
Units: seconds at MIPEAK Default: 1200
Opmodes: all Drive Status: en/dis EEPROM: yes