### DIP

displays the settings of the DIP switches located on top of the drive. This variable returns a series of 1’s and 0’s for each of the switches, with a comma inserted in the middle for clarity. Switch 10 is the leftmost digit, and switch 1 is the rightmost.

Note: in firmware versions prior to V2.0.0, there were only 8 DIP switches, and no comma was printed out.

Firmware Versions: all
Type: switch mode (R)
Range: 00000000-11111111 (firmware versions prior to 2.0.0)
00000,00000-11111,11111 (firmware 2.0.0 and later)
Units: 1=on, 0=off Default: hardware defined
Opmodes: all Drive Status: en/dis EEPROM: no