### MSININT

is used with the sine encoder option and sets the interpolation level of the sine encoder.

The total sine encoder feedback resolution is (MENCRES * MSININT) lines per rev (before quadrature).

Firmware Versions: 3.2.0 (3.3.0 Variable is automatically set to 256)
Type: switch mode (R/W) Range: 1, 2, 4, 8, 16, 32, 64, 128, 256, 512, 1024, 2048, 4096 (for EnDat encoders or software sine interface)
Range: 256 only (for all other sine encoders)
Units: bits Default: 256
Opmodes: all Drive Status: dis EEPROM: yes