### MEMW

Read or write a word in the HPC memory.
Syntax:

MEMW <addr> <value>
<addr> - HPC memory location. Range: 0 to 65535, even values.
<value> - optional. If specified, write operation is performed. If not specified, read operation is performed. Range: 0 to 65535.

memw haddr - querries the hexadecimal address "addr".
memw haddr value - Sets the "value" into the "addr" address.

See also: MEMB , DMEML

Firmware Versions: all
Command Syntax: See above
Opmodes: all , Drive Status: en/dis