### SININIT

triggers the sine calibration process.

0 = cancels the sine calibration process.
1 = starts the sine calibration process.
The sine calibration process is applicable for software sine encoder or software resolver feedback.

If calibrates (nulls) the offset of the sine and cosine signals, and it finds the gain that matches the amplitude of those signals.

In software resolver feedback it also finds the gain that scales the amplitudes of the sine and cosine signals to maximum.

For more details, see SININITST and SINPARAM.

Firmware Versions: 6.2.0 and later
Type: switch (R/W) Range: 0, 1
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: no