### ANLPFHZ

sets a filter rate (corner frequency) for the analog input filter. This is a simple single pole filter which is always present. The filter rate adjusts automatically as the analog input sampling rate changes for different operational modes. A value of 10,000 = unity gain (no filter).

Firmware Versions: 2.1.0 and later
Type: variable (R/W) Range: 1 to 10,000
Units: Hz Default: 10,000
Opmodes: 1,3,8 Drive Status: en/dis EEPROM: yes