### MEMB

Read or write a byte in the HPC memory.
Syntax:

MEMB <addr> <value>
<addr> - HPC memory location. Range: 0 to 65535.
<value> - optional. If specified, write operation is performed. If not specified, read operation is performed. Range: 0 to 255.

memb haddr - querries the hexadecimal address "addr".
memb haddr value - Sets the "value" into the "addr" address.

See also: MEMW , DMEML

Firmware Versions: all
Command Syntax: See above
Opmodes: all , Drive Status: en/dis