### DUMP

transmits all variables and their settings to the serial port terminal. This command actually outputs the EEPROM contents of the drive to the serial port, where the variables can then be reviewed or saved to a variable file (*.SSV).
Since version 3.7.0 an additional functionality has been added. DUMP response is broken into parts according to an additional optional parameter.This is useful for hosts with limited amount of buffer. a pound sign '#' indicates the end of the list, followed by the prompt.

Firmware Versions: all , revised from 3.7.0
Command Syntax: DUMP {N-lines}
N-lines (optional): 1 to 1000 in lines
Opmodes: all Drive Status: en/dis