### e 1 0 3 - DSP load fail (during init)

We have had quite a few cases of the CD Series 5 drive going into watchdog at power up, with the display showing E102-E104 and then WD.

Version 7.3.3q, to be used in applications in place of 7.3.3. This version has exactly the same functionality of 7.3.3. The Altera image has been compiled with the QuartusII compiler instead of the MaxplusII compiler, since this has been found to fix the E102-E104-WD problem.

Full Report