### MLMIN

sets the motor’s minimum line-to-line inductance. This variable is used for current loop controller design and as an input to the Torque Angle Control algorithms. When this variable is changed, the drive will enter a no-comp state, requiring a CONFIG command (see CONFIG).

Firmware Versions: all
Type: variable (R/W) Range: 1 to 32767
Units: millihenries *10^-2 Default: motor data
Opmodes: all Drive Status: dis EEPROM: yes