### CLREEPROM

clears the non-volatile memory (EEPROM) in the drive and resets all variables (drive/motor/operational) to their factory defaults. The drive null’s the EEPROM and recovers from a NVRAM error and assumes a no-comp state. A complete drive configuration procedure then has to be initiated before resuming drive operation. This command is the only method of resetting the run time clock (see TRUN).

Firmware Versions: all
Command Syntax: CLREEPROM
Opmodes: all Drive Status: dis