### THERMTRIP

set the motor thermostat voltage trip level. There is a circuit that converts the motor thermostat resistance into voltage. When this voltage crosses THERMTRIP level, the motor thermostat is considered opened.

This command is password protected.

Firmware Versions: all
Type: variable (R/W) Range: 0 to 5000
Units: millvoltes Default: 3500
Opmodes: all Drive Status: en/dis EEPROM: yes