### MFOLDT

sets the time constant for motor foldback. After the drive enters the motor foldback state (MFOLD=1), this variable defines how long it will take the drive to reduce the system current level to MICONT. See also FOLD, FOLDD, FOLDR, FOLDT, FOLDMODE, FOLDTIME, MFOLD, MFOLDD, MFOLDDIS, and MFOLDR.

Firmware Versions: 3.2.0 and later
Type: variable (R/W) Range: 1 to 1200
Units: seconds Default: 600
Opmodes: all Drive Status: en/dis EEPROM: yes