### MAPOS

sets the absolute position for INxMODE 13. Position is in counts, where 65536 counts represent one motor revolution for resolver systems, and 4*MENCRES counts represents on motor revolution for encoder systems.

When IN1MODE, IN2MODE, or IN3MODE is set equal to 13, and the associated digital input (IN1, IN2, or IN3) goes high, the drive will move to MAPOS at a speed of MASPEED.

Firmware Versions: 3.1.0 and later
Type: variable (R/W) Range: +/- 2,147,483,647
Units: counts Default: 0
Opmodes: 8 Drive Status: en/dis EEPROM: yes