### DEADTIME

PWM dead time (to avoid the short of the IPM).
In the past the deadtime was activated by Digital Board ALTERA. Now it is controlled by Power Board ALTERA and this command does not work.
Appears in the command list, but has no function in the drive.

This command is password protected.

Firmware Versions: all
Type: variable (R/W) Range: -63 to 63
Units: 0.1 usec Default: hardware defined (As usual 0, 35 for "vector star")
Opmodes: all Drive Status: dis EEPROM: yes