### MSINFRQ

sets the maximum frequency limit of the encoder equivalent output in case of sine encoder option board, software sine encoder interface, or software resolver interface. If the encoder equivalent output exceeds the value set by this variable, it becomes inaccurate, and a burst overflow fault is generated.
0 = ignore burst overflow fault
1 = 2.5 MHz
2 = 1.25 MHz
3 = 625 KHz
4 = 312 KHz

Firmware Versions: 3.3.0
Type: switch mode (R/W) Range: 0-4
Units: n/a Default: 1
Opmodes: all Drive Status: dis EEPROM: yes